**SECTION 310 WASHROOM AND TOILET ROOM REQUIREMENTS   
  
310.1 Light and ventilation.**   
Washrooms and toilet rooms shall be illuminated and ventilated in accordance with the *International Building Code* and *International Mechanical Code.*  **310.2 Location of fixtures and compartments.**   
The location of plumbing fixtures and the requirements for compartments and partitions shall be in accordance with [Section 405.3.](javascript:Next('./icod_ipc_2012_4_par026.htm');)  **310.3 Interior finish.**   
Interior finish surfaces of toilet rooms shall comply with the *International Building Code.*