**SECTION 401 GENERAL   
  
401.1 Scope.**   
This chapter shall govern the materials, design and installation of plumbing fixtures, faucets and fixture fittings in accordance with the type of *occupancy*, and shall provide for the minimum number of fixtures for various types of occupancies.  **401.2 Prohibited fixtures and connections.**   
Water closets having a concealed trap seal or an unventilated space or having walls that are not thoroughly washed at each discharge in accordance with ASME A112.19.2/CSA B45.1 shall be prohibited. Any water closet that permits siphonage of the contents of the bowl back into the tank shall be prohibited. Trough urinals shall be prohibited.  **401.3 Water conservation.**   
The maximum water flow rates and flush volume for plumbing fixtures and fixture fittings shall comply with [Section 604.4.](javascript:Next('./icod_ipc_2012_6_par020.htm');)