**SECTION 407 BATHTUBS

407.1 Approval.**
Bathtubs shall conform to ANSI Z124.1.2, ASME A112.19.1/CSA B45.2, ASME A112.19.2/CSA B45.1, ASME A112.19.3/CSA B45.4 or CSA B45.5.  **407.2 Bathtub waste outlets and overflows.**
Bathtubs shall be equipped with a waste outlet and an overflow outlet. The outlets shall be connected to waste tubing or piping not less than 11/2 inches (38 mm) in diameter. The waste outlet shall be equipped with a water-tight stopper.  **407.3 Glazing.**
Windows and doors within a bathtub enclosure shall conform to the safety glazing requirements of the *International Building Code*.  **407.4 Bathtub enclosure.**
Doors within a bathtub enclosure shall conform to ASME A112.19.15.