**SECTION 408 BIDETS

408.1 Approval.**
Bidets shall conform to ASME A112.19.2/CSA B45.1.  **408.2 Water connection.**
The water supply to a bidet shall be protected against backflow by an *air gap* or backflow preventer in accordance with Section 608.13.1, 608.13.2, 608.13.3, 608.13.5, 608.13.6 or 608.13.8.  **408.3 Bidet water temperature.**
The discharge water temperature from a bidet fitting shall be limited to a maximum temperature of 110°F (43°C) by a water temperature limiting device conforming to ASSE 1070 or CSA B125.3.