**SECTION 408 BIDETS   
  
408.1 Approval.**   
Bidets shall conform to ASME A112.19.2/CSA B45.1.  **408.2 Water connection.**   
The water supply to a bidet shall be protected against backflow by an *air gap* or backflow preventer in accordance with [Section 608.13.1](javascript:Next('./icod_ipc_2012_6_par148.htm');), [608.13.2](javascript:Next('./icod_ipc_2012_6_par149.htm');), [608.13.3](javascript:Next('./icod_ipc_2012_6_par150.htm');), [608.13.5](javascript:Next('./icod_ipc_2012_6_par152.htm');), [608.13.6](javascript:Next('./icod_ipc_2012_6_par153.htm');) or [608.13.8.](javascript:Next('./icod_ipc_2012_6_par155.htm');)  **408.3 Bidet water temperature.**   
The discharge water temperature from a bidet fitting shall be limited to a maximum temperature of 110°F (43°C) by a water temperature limiting device conforming to ASSE 1070 or CSA B125.3.