**SECTION 414 GARBAGE CAN WASHERS   
  
414.1 Water connection.**   
The water supply to a garbage can washer shall be protected against backflow by an *air gap* or a backflow preventer in accordance with [Section 608.13.1](javascript:Next('./icod_ipc_2012_6_par148.htm');), [608.13.2](javascript:Next('./icod_ipc_2012_6_par149.htm');), [608.13.3](javascript:Next('./icod_ipc_2012_6_par150.htm');), [608.13.5](javascript:Next('./icod_ipc_2012_6_par152.htm');), [608.13.6](javascript:Next('./icod_ipc_2012_6_par153.htm');) or [608.13.8.](javascript:Next('./icod_ipc_2012_6_par155.htm');)  **414.2 Waste connection.**   
Garbage can washers shall be trapped separately. The receptacle receiving the waste from the washer shall have a removable basket or strainer to prevent the discharge of large particles into the drainage system.