**SECTION 415 LAUNDRY TRAYS   
  
415.1 Approval.**   
Laundry trays shall conform to ANSI Z124.6, ASME A112.19.1/CSA B45.2, ASME A112.19.2/CSA B45.1, ASME A112.19.3/CSA B45.4.  **415.2 Waste outlet.**   
Each compartment of a laundry tray shall be provided with a waste outlet not less than 11/2 inches (38 mm) in diameter and a strainer or crossbar to restrict the clear opening of the waste outlet.