**SECTION 416 LAVATORIES   
  
416.1 Approval.**   
Lavatories shall conform to ANSI Z124.3, ASME A112.19.1/CSA B45.2, ASME A112.19.2/CSA B45.1, or ASME A112.19.3/CSA B45.4. Group wash-up equipment shall conform to the requirements of [Section 402](javascript:Next('./icod_ipc_2012_4_par004.htm');). Every 20 inches (508 mm) of rim space shall be considered as one lavatory.  **416.2 Cultured marble lavatories.**   
Cultured marble vanity tops with an integral lavatory shall conform to ANSI Z124.3 or CSA B45.5.  **416.3 Lavatory waste outlets.**   
Lavatories shall have waste outlets not less than 11/4 inches (32 mm) in diameter. A strainer, pop-up stopper, crossbar or other device shall be provided to restrict the clear opening of the waste outlet.  **416.4 Moveable lavatory systems.**   
Moveable lavatory systems shall comply with ASME A112.19.12.  **416.5 Tempered water for public hand-washing facilities.**  *Tempered water* shall be delivered from lavatories and group wash fixtures located in public toilet facilities provided for customers, patrons and visitors. *Tempered water* shall be delivered through an *approved* water-temperature limiting device that conforms to ASSE 1070 or CSA B125.3.