**SECTION 418 SINKS   
  
418.1 Approval.**   
Sinks shall conform to ANSI Z124.6, ASME A112.19.1/CSA B45.2, ASME A112.19.2/CSA B45.1 or ASME A112.19.3/CSA B45.4.  **418.2 Sink waste outlets.**   
Sinks shall be provided with waste outlets having a diameter not less than 11/2 inches (38 mm). A strainer or crossbar shall be provided to restrict the clear opening of the waste outlet.  **418.3 Moveable sink systems.**   
Moveable sink systems shall comply with ASME A112.19.12.