**SECTION 505 INSULATION

[E] 505.1 Unfired vessel insulation.**
Unfired hot water storage tanks shall be insulated to R-12.5 (h • ft2 • °F)/Btu (R-2.2 m2 • K/W).