**ICC PLUMBING CODE SECTION 611 DRINKING WATER TREATMENT UNITS   
  
611.1 Design.**   
Drinking water treatment units shall meet the requirements of NSF42, NSF 44, NSF 53, NSF 62 or CSA B483.1.  **611.2 Reverse osmosis systems.**   
The discharge from a reverse osmosis drinking water treatment unit shall enter the drainage system through an *air gap* or an *air gap* device that meets the requirements of NSF 58 or CSA B483.1.  **611.3 Connection tubing.**   
The tubing to and from drinking water treatment units shall be of a size and material as recommended by the manufacturer. The tubing shall comply with NSF 14, NSF 42, NSF 44, NSF 53, NSF 58 or NSF 61.