**SECTION 707 PROHIBITED JOINTS AND CONNECTIONS   
  
707.1 Prohibited joints.**   
The following types of joints and connections shall be prohibited:

1. Cement or concrete joints.

2. Mastic or hot-pour bituminous joints.

3. Joints made with fittings not *approved* for the specific installation.

4. Joints between different diameter pipes made with elastomeric rolling O-rings.   
  
5 Solvent-cement joints between different types of plastic pipe.

6. Saddle-type fittings.