**SECTION 310 WASHROOM AND TOILET ROOM REQUIREMENTS

310.1 Light and ventilation.**
Washrooms and toilet rooms shall be illuminated and ventilated in accordance with the *International Building Code* and *International Mechanical Code.*  **310.2 Location of fixtures and compartments.**
The location of plumbing fixtures and the requirements for compartments and partitions shall be in accordance with Section 405.3.  **310.3 Interior finish.**
Interior finish surfaces of toilet rooms shall comply with the *International Building Code.*