**ICC PLUMBING CODE SECTION 613 TEMPERATURE CONTROL DEVICES AND VALVES   
  
613.1 Temperature-actuated mixing valves.**   
Temperature-actuated mixing valves, which are installed to reduce water temperatures to defined limits, shall comply with ASSE 1017.